WAN Subnet Info:IP : 38.140.54.125 Net Mask : 255.255.255.248IP Gateway : 38.140.54.121ISP DNS: 66.28.0.45ISP DNS: 66.28.0.61Midtown DNS: 10.1.10.10Midtown DNS: 10.254.10.10Local Subnet: 10.58.1.0 255.255.255.0Internal (Port1): 10.58.1.1 255.255.255.0DMZ(Enable PING,HTTPS,SSH,FMG\_ACCESS,RADIUS-ACCT,FTM,FORTITELEMETRY)VPN\_COR1VPN\_COR2VPN\_DR1Wireless\_private > Internal 1Wireless\_public TFTP/SCP file copy to flash for CiscoUpgrade the device to 6.0.4Upgrade pathDHCP Options Config system dhcp server edit 1 set start-ip 10.58.1.100 set end-ip 10.58.1.253 edit 2 set interface "dmz" config ip-range edit 1 set start-ip 10.58.4.2 set end-ip 10.58.4.254 next endCONF File > configurationOUT File > firmware